what if I print the black outline of the circuit connections.

what if the paper that is black is then illuminated.

Since it is black, it will get hotter faster than the white portions.

What if I spray, sprinkle, or otherwise apply conductive material to the now hot portions.

What about aluminum foil or aluminum oxide. It has 0.625 the conductance of copper.