What I want to do.

I want to build 2 receivers and with those receivers produce the hyperboloid of an actual radio source that I select by tuning.

The receivers will be remotely located and controlled over the internet.

This will look like two softare defined receivers, in different locations, controlled over the internet.

They will each look at a source at the same frequency in analog RF.

-----------------

I want to tune two receivers remotely to listen for the same frequency.

They will record RF for some interval.

They will transmit those recordings to a comparator that will determine the delay between the two recordings.

That single delay value will produce a hyperboloid surface drawn in relation to the two receivers.

That delay value along witht the known geometry of the receivers will be sent to the user on the internet.

The user will run a program that will draw the hyperboloid for those two receivers.

----------------

i want to tune three receivers remotely to listen for the same frequency.

The will record three streams of RF for some interval

The will tranmit these recordings to two comparators that will determine the two delays between the three recordings.

Those two delay values will produce two hyperboloid surfaces which can be intersected to form a curve

---------

Add the union and intersection of two circles in geometry expressions to math book.