use a set of cheap A/D converters clocked in offset to sample a high frequency signal.

tune by bringing additional converters in and out of the picture.