purepath notes

1) Only the TAS3204 Processor is relevant for my application unless I split up the functions, which could be desirable for concurrency and band filtering.

2) no FFT ;-(  even for monitoring.

3) output is ASM... if output had been C, it would have been much more widely applicable.

4) draw system diagram

try several mappings

write report

provide summary to Joey and "tricia".

remove software from machine if not applicable and report having done so.

See if you can accomplish this by

mono voice and test chirps --> multiply by carrier ---> filter alias ---> amplify --> broadcast

stereo ears --> downconvert --> filter --> amplify --> listen